force = 70 # kg (person’s weight)

displacement = 0.002 # m (tile depression)

piezo\_efficiency = 0.3 # 30% efficiency

energy = force \* displacement \* piezo\_efficiency \* 1000 # мДж

print(f"Generated energy: {energy:.2f} мДж")